Rockwell Commander 500s Shrike
REFERENCE INFORMATION

Total Flight Simulator aircraft weight with full fuel | 6,750 Lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

V2 – Take off Speed | 95 MPH
VA - Maneuvering Speed | 163 MPH
VLO - Maximum Gear Operating Speed | 180 MPH
VLE - Maximum Landing Gear Extension Speed | 180 MPH
VNO Maximum Structural Cruising Speed | 230 MPH
VNE - Never Exceed Speed | 288 MPH
Vsi - Stalling Speed (maximum weight) | 78 MPH
VSO - Stalling Speed in Landing Configuration | 68 MPH
VX - Two-engine Best Angle-of-Climb Speed | 97 MPH
VY - Two-engine Best Rate-of-Climb Speed | 110 MPH
VXSE - Single-engine Best Angle-of-Climb Speed | 95 MPH
VYSE - Single-engine Best Rate-of-Climb Speed | 101 MPH
VMC - Minimum Control Speed-Single Engine | 75 MPH
Minimum Glide Range Speed | 125 MPH

Maximum Flap Placard Speeds

Flaps degrees | MPH
10 | 180
20 | 150
30 | 135
40 | 135

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.