Hi all
Here are the Installation Instructions in easy, basic and advanced versions. Use the easy version for a quick and easy 
install (hence the name easy), you can also use the basic installation method if the easy method does not work.
Use the advanced method if you have edited the CLS Piper Arrow flight model or have already added textures to the aircraft.
Here are the instructions below:

EASY

1) If you have not done so already Download and Install the CLS Piper Arrow.
2) Open the folder entitled "easy"
3) Run the CLS Piper arrow CIX Repaint.exe file as an administrator (Vista, and Windows 7 Only)
4) Follow the On-Screen Instructions

BASIC

1) If you have not done so already Download and Install the CLS Piper Arrow.
2) Open the folder entitled "Basic"
3) Copy and Paste the texture.cix folder and its contents into the CLS_piperarrow folder. 
(In C:\Program Files (x86)\Microsoft Games\Microsoft Flight Simulator X\SimObjects\Airplanes\CLS_piperarrow as default)
4) Copy and Paste and Overwrite the aircraft.cfg file into the same CLS_piperarrow Folder.


ADVANCED

1) If you have not done so already Download and Install the CLS Piper Arrow.
2) Open the folder entitled "Advanced"
3) Copy and Paste the texture.cix folder and its contents into the CLS_piperarrow folder.
(In C:\Program Files (x86)\Microsoft Games\Microsoft Flight Simulator X\SimObjects\Airplanes\CLS_piperarrow as default) 
4) Open the aircraft.cfg in the CLS_piperarrow folder with notepad or another text editor.
5) Scroll down to the last [fltsim.XX] entry (in the XX will be a number).
6) Copy and paste this below the last [fltsim.XX] entry:

[fltsim.XX]
title=Commercial Level Simulations -- Piper PA-28R-200 Arrow II CIX
sim=Piper_PA28R_Arrow
model=
panel=blu
sound=
texture=cix

kb_checklists=Piper_PA28R_Arrow_Chk
kb_reference=
atc_id=G-CIXV

ui_typerole="Single Engine Prop"
ui_createdby="Commercial Level Simulations"
ui_manufacturer="Commercial Level Simulations"
ui_type=Piper PA-28R-200 Arrow II
ui_variation=CIX colours (G-CIXV)

description=Created by Commercial Level Simulations\nRepainted in CIX colours by Samuel White\nPiper PA-28R-200 Arrow II\nVersion FSX-2007.1.0\n\nFuel Capacity:   72 gal\/182 l\nStall Speed:       53 kts (dirty)\nMax TAS:           145 kts\nCruise TAS:      137 kts (75% power)\nCruise Range:   880 nm\/1,1630 km (with 45 min reserve)\n\nService Ceiling (100 fpm): 16,200 ft\/3,353 m\nRate of Climb:    649 fpm\n\nTakeoff\nGround Roll: 1065 ft\nOver 50ft Obstacle: 1760 ft

6) change the XX in the [fltsim.XX] to the next number shown in the sequence of [fltsim.XX] entries.
7) Save the File in the same folder. (If an Vista or Windows seven user go to instruction 8, if not you have finished the 
instillation)
8) Save the File in my documents.
9) Copy and Paste the file you saved in my documents into the CLS_piperarrow Folder and overwrite the previous one.


I would like to thank Peter Dodds, and everyone else for helping me with creating this repaint, and giving me ideas
 of what to add to it next.I Hope You enjoy using this Repaint as much as I enjoyed creating it!!!

P.S If you see any problems with this file please feel free to email me at: sam.white1011@gmail.com
