## Seabird SB7L Seeker Specifications

External Dimensions
Wing Span | 11.07 m | 36 ft 4 in
Overall Length | 7.00 m | 23 ft 0 in
Height of Vertical Stabiliser | 2.03 m | 6 ft 7 in
Wheelbase | 2.04 m | 6 ft 8 in
Internal Dimensions
Cabin Width | 1.12 m | 3 ft 8 in
Doors - Long Axis | 1.07 m | 3 ft 6 in
Weights
Empty weight | 610kg | 1342 lb
Maximum T/O Mass | 925 kg | 2040 lb
Speeds
Min Patrol Speed (CAS) | 121 km/h | 65 kts
Cruise 75% Power (CAS) | 208 km/h | 112 kts
Never Exceed (CAS) | 239 km/h | 129 kts
Stall (40° Flap)(IAS) | 89 km/h | 48 kts
Fuel Capacity
Usable | 180 litres | 47.5 US gal
Endurance (inc. reserve)
Min. Patrol Speed | 65 kts | 7 h 15 min
Cruise (65% Power) |  | 4 h 30 min
Range
Patrol Speed (65 kts) | 880 km | 476 nm
Cruise (65% Power) | 869 km | 470 nm
Fuel Flow
Patrol Speed (65 kts) | 22 l/h | 5.80 US gal/h
Cruise (65% Power) | 34 l/h | 9.00 US gal/h
Take-off/Landing run at AUW
T-O run | 264 m | 870 ft
Landing run | 198 m | 654 ft