SOPWITH CAMEL PROCEDURES

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For suggested speeds, see the Reference tab.

____________________________________

ENGINE START

Press CTRL+E to initiate engine autostart sequence

____________________________________

TAKEOFF

[ ] Throttle -- FULL

(press F4)

[ ] Elevator Control -- PUSH FORWARD ON STICK

(until tail comes up)

-- At 55 KIAS, EASE BACK ON STICK

____________________________________

CLIMB

[ ] Climb Speed -- 60 KIAS or greater

____________________________________

CRUISE

[ ] Throttle -- 1200 RPM

(press F2 or F3 as necessary)

____________________________________

DESCENT

[ ] Throttle -- 800 RPM

(press F2 or F3 as necessary)

____________________________________

LANDING

[ ] Airspeed -- 60 KIAS

[ ] Throttle -- AS NECESSARY to adjust descent rate

(press F2 or F3 as necessary)

[ ] Touchdown -- MAIN WHEELS FIRST

[ ] Landing Roll -- LOWER TAILSKID GENTLY

[ ] Elevator Control -- HOLD STICK FULLY BACK

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator X / Prepar3d. To learn about using, printing, and customizing checklists, see Help.