De Havilland Chipmunk T10

Please see Panel Manual for controls

To... | Press...
Display/hide Radio | SHIFT+2
Display/hide GPS | SHIFT+3
Display/hide Electrical panel | SHIFT+4
Display/hide Compass | SHIFT+5
Display/hide Fuel panel | SHIFT+6
Display/hide "G" Meter | SHIFT+7
Display/hide Throttle/Mixture | SHIFT+8

BEFORE STARTING ENGINE |
[ ] Brakes | TEST AND SET (press CTRL+PERIOD key)
[ ] Electrical Equipment, | OFF
[ ] Master Switch | OFF
ENGINE START |
Press CTRL+E to initiate engine autostart sequence, or:
[ ] Throttle | Closed (press F1 as necessary)
[ ] Mixture | RICH press CTRL+SHIFT+F3 until full forward
[ ] Propeller Area | CLEAR
[ ] Avionics Master Switch | ON
[ ] Master Switch | ON
[ ] Ignition Switch | START (release when engine starts) (press M+PLUS key to R, L, Both, Start)
Then: |
[ ] Oil Pressure | CHECK
[ ] Nav Lights | ON as required
[ ] Master Switch | ON
[ ] Flaps | RETRACT (press F6 until Up)
BEFORE TAKEOFF |
[ ] Parking Brake | SET (press CTRL+PERIOD)
[ ] Flight Controls | FREE AND CORRECT
[ ] Flight Instruments | CHECK and SET
[ ] Fuel Quantity | CHECK
[ ] Mixture | RICH (press CTRL+SHIFT+F3 until fully in)
[ ] Elevator Trim | SET for takeoff (with Num Lock off, press Num Pad 1 or Num Pad 7 as necessary)
[ ] Throttle | 1500 RPM (press F3 or F2 as necessary)
[ ] Magnetos | CHECK <150 RPM drop on each; <50 RPM drop between (press M+MINUS key, then press M+PLUS key to L, R, L, Both)
[ ] Engine Instruments | CHECK
[ ] Throttle | 1000 RPM or less (press F2 or F3 as necessary)
[ ] Radio | SET (press SHIFT+2 to display radio stack)
[ ] Wing Flaps | SET for takeoff (0-15 degrees) (press F7 or F6 as necessary)
[ ] Brakes | RELEASE (press PERIOD key)
TAKEOFF |
[ ] Wing Flaps | 0-15 degrees (press F7 or F6 as necessary)
[ ] Throttle | FULL OPEN (press F3 until fully forward)
[ ] Carb Heat | ON press H
[ ] Mixture | RICH (above 3000 feet, LEAN to obtain maximum RPM) (press CTRL+SHIFT+F3 or CTRL+SHIFT+F2 as necessary)
[ ] Climb Speed | 65-70 KIAS
EN ROUTE CLIMB |
[ ] Airspeed | 65-70 KIAS
[ ] Throttle | FULL OPEN/as required (press F3 as necessary)
[ ] Mixture | RICH (above 3000 feet, LEAN to obtain maximum RPM) (press CTRL+SHIFT+F3 or CTRL+SHIFT+F2 as necessary)
CRUISE |
[ ] Power | (1900 RPM gives approx 90 kts) (press F2 or F3 as necessary)
[ ] Elevator Trim | ADJUST (with Num Lock off, press Num Pad 1 or Num Pad 7 as necessary)
[ ] Carb Heat | OFF as necessary) press H
[ ] Mixture | LEAN (press CTRL+SHIFT+F2 or CTRL+SHIFT+F3 as necessary)
DESCENT |
[ ] Power | AS DESIRED (press F2 or F3 as necessary)
[ ] Carb Heat | ON
[ ] Mixture | ADJUST for smooth operation (Full Rich for idle power) (press CTRL+SHIFT+F3 as necessary)
BEFORE LANDING |
[ ] Mixture | RICH (press CTRL+SHIFT+F3 as necessary)
[ ] Landing/Taxi Lights | ON
LANDING |
[ ] Airspeed | 70 KIAS (flaps UP)
[ ] Wing Flaps | AS DESIRED 0-15 degrees <85 KIAS 15-30 degrees <70 KIAS (press F6 or F7 as necessary)
[ ] Airspeed | 5 0-60 KIAS (flaps DOWN)
[ ] Touchdown | MAIN WHEELS FIRST
[ ] Landing Roll | LOWER TAIL WHEEL GENTLY
[ ] Braking | MINIMUM REQUIRED (press PERIOD key)
AFTER LANDING |
[ ] Carb Heat | OFF
[ ] Wing Flaps | UP (press F6 as necessary)
SECURING AIRPLANE |
[ ] Parking Brake | SET (press CTRL+PERIOD)
[ ] Nav Lights | OFF
[ ] Landing/Taxi Lights | OFF
[ ] Avionics Master Switch, Electrical Equipment, | OFF
[ ] Mixture | IDLE CUT OFF (press CTRL+SHIFT+F2 until fully out)
[ ] Ignition Switch | OFF (press M+MINUS key until Off)
[ ] Master Switch | OFF

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.