EXTRA 300S
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 8,750 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.
Speeds are given for Normal (2,028 lbs) and Aerobatic (1,808 lbs).

VA - Maneuvering Speed (normal) | 140 KIAS
VA - Maneuvering Speed (aerobatic) | 158 KIAS
VA - Maneuvering Speed (6,250 lbs) | 112 KIAS
VNO - Max Structural Cruising Speed | 158 KIAS
VNE - Never Exceed Speed | 220 KIAS
VS - Stalling Speed (normal) | 59 KIAS
VS - Stalling Speed (aerobatic) | 55 KIAS
VX - Best Angle-of-Climb Speed (normal) | 93 KIAS
VX - Best Angle-of-Climb Speed (aerobatic) | 87 KIAS
VY - Best Rate-of-Climb Speed (normal) | 104 KIAS
VY - Best Rate-of-Climb Speed (aerobatic) | 96 KIAS
Best Glide Speed (normal) | 90 KIAS
Best Glide Speed (aerobatic) | 80 KIAS

Recommended Aerobatic Maneuver Entry Speeds

Maneuver | Min Speed | Max Speed
45-degree climb | 80 KIAS | VNO
90-degree climb | 158 KIAS | VNO
45-degree dive | VS | VNO
90-degree dive | VS | VNO
1/4 loop climb | 100 KIAS | 190 KIAS
Loop | 100 KIAS | 190 KIAS
Stall turn | 100 KIAS | 190 KIAS
Aileron roll | 80 KIAS | 158 KIAS
Snap roll | 80 KIAS | 140 KIAS
Tail slide | 100 KIAS | 190 KIAS
Knife edge | >150 KIAS | VNO
Inverted flight | >VS | 190 KIAS

Load Factor Limitations
+6 G / -3 G (normal)
+10 G / -10 G (aerobatic)

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.